1. Remove the retractor mounting bolt (A) and the retractor bolt (B), then remove the rear seat belt (C) and retractor (D).

1. Install the seat belt in the reverse order of removal, and note these items:
   - Check that the retractor locking mechanism functions as described.
   - Tighten the bolts by hand first, then tighten to specification with a torque wrench.
   - Before installing the anchor bolt, make sure there are no twists or kinks in the rear seat belt.