Countershaft

Item | Measurement | Qualification | Standard or New | Service Limit
--- | --- | --- | --- | ---
Countershaft | Diameter of needle bearing contact area | At torque converter housing | 36.005−36.015 mm (1.4175−1.4179 in.) | When worn or damaged
At 4th gear | 34.982−34.998 mm (1.3772−1.3779 in.) | When worn or damaged
At reverse gear collar | 39.979−40.000 mm (1.5740−1.5748 in.) | When worn or damaged
I.D. of gears | 4th gear | 41.000−41.016 mm (1.6142−1.6148 in.) | When worn or damaged
Reverse gear | 46.000−46.016 mm (1.8110−1.8116 in.) | When worn or damaged
End play of gears | 5th gear | 0−0.48 mm (0−0.019 in.) | ———
4th gear | 0.04−0.27 mm (0.001−0.011 in.) | ———
Reverse gear | 0.10−0.25 mm (0.004−0.010 in.) | ———
Collar, 35 x 47 x 7.8 mm thickness |  | 7.8 mm (0.31 in.) | ———
Distance collar length |  | 57.75−57.80 mm (2.274−2.276 in.) | ———
Reverse selector hub width |  | 25.45−25.65 mm (1.002−1.010 in.) | ———
Reverse selector hub O.D. |  | 55.87−55.90 mm (2.200−2.201 in.) | When worn or damaged