Maintenance Schedule for Normal Conditions - Australia and New Zealand
100,000km(5year)

Follow the Normal Conditions Maintenance Schedule if the severe driving conditions specified in the Severe Conditions Maintenance Schedule do not apply.

Service at the indicated distance or time whichever comes first

| Replace engine oil filter

| Replace spark plugs

| Inspect idle speed

| Check front and rear brakes

|  | Check the brake pad and disc thickness. Check for damage or cracks.
|  | Check the calipers for damage, leaks, and tightness.

| Check lights alignment

Check the position of the headlights.

| Test drive (noise, stability, dashboard operation)

| Tie-rod ends, steering gearbox, and boots

|  | Check rack grease and steering linkage.
|  | Check the boot for damage and leaking grease.

| Suspension components

|  | Check the bolts for tightness.
|  | Check all dust cover for deterioration and damage.

| Driveshaft boots

|  | Check the boot and boot band for cracks.
|  | Check rack grease.

| Brake hoses and lines (including VSA lines)

Check the master cylinder and VSA modulator-control unit and leakage.

| All fluid levels and condition of fluids

Check levels and check for leaks. If necessary, add.

|  | Engine coolant
|  | MTF
|  | ATF
|  | Clutch fluid
|  | Power steering fluid
|  | Brake fluid
|  | Windshield fluid

| Exhaust system

Check the exhaust pipe and muffler for damage, leaks, and tightness.

| Fuel lines and connections

|  | Check fuel lines for loose connections, cracks, and deterioration.
|  | Retighten loose connections and replace any damaged parts.

Every 10,000 km or 1 year

| Replace engine oil

At 200,000 km or 10 years, then every 100,000 km or 5 years

| Replace engine coolant

Use genuine Honda All Season Antifreeze/Coolant Type 2.

At 120,000 km or 6 years, then every 80,000 km or 4 years

| Replace Automatic Transmission Fluid (ATF)

Use genuine Honda ATF-Z1.

Every 3 years

| Replace brake fluid

|  | Use only DOT 3 or DOT 4 brake fluid. We recommend genuine Honda Brake Fluid.
|  | Check that brake fluid level between the upper and lower marks on the reservoir.

Every 30,000 km (18,750 miles) or 1 year

| Replace dust and pollen filter

Every 10,000 km

| Rotate tyres (Check tyre inflation and condition at least once per month)