DTC Troubleshooting: 107

DTC 107: Millimeter Wave Radar Unit Aiming Incomplete NOTE: If the millimeter wave radar unit is removed or replaced, it is necessary to aim it, otherwise DTC 107 is stored even if the system is OK.

1. Turn the ignition switch ON (II), and watch the adaptive cruise control (ACC) indicator.

Does the adaptive cruise control (ACC) indicator stay off?

YES | - | Intermittent failure, the system is OK at this time.■
NO | - | Go to Step 2 .

1. Check for DTCs with the HDS.

Is DTC 107 indicated?

YES | - | If DTC 107 is indicated again after the aiming is complete, check for loose or poor connection. If OK, replace the millimeter wave radar unit. ■
NO | - | Go to Step 3 .

1. Check for DTCs with the HDS.

Are any DTCs indicated?

YES | - | Troubleshoot the indicated DTC.■
NO | - | Check for loose or poor connection. If OK, replace the adaptive cruise control (ACC) unit, then go to Step 4 .

1. Check for DTCs with the HDS.

Is DTC 107 indicated?

YES | - | Check for loose or poor connection. If OK, replace the millimeter wave radar unit. ■
NO | - | Troubleshoot the indicated DTC. If there is no DTC, the system is OK at this time.■