DTC P1384: Glow Plug Circuit Malfunction

1. Turn the ignition switch ON (II).

1. Clear the DTC with the HDS.

1. Do the GLOW PLUG TEST in the INSPECTION MENU with the HDS.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P1384 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the glow plug control module and the ECM.■

1. Turn the ignition switch OFF.

1. Disconnect the glow plug control module 11P connector.

1. Measure resistance continuity between body ground and glow plug control module 11P connector terminals No. 1, No. 2, No. 3, and No. 4 individually.

Is there about 1.0 Ω?

YES | - | Go to Step 8 .
NO | - | Repair open in the wire between the glow plug control module and each glow plug, then go to Step 11 .

1. Disconnect all glow plugs 1P connector.