1. Remove the rear mount stop (A), then remove the rear mount bolt (B).

1. Check that the engine/transmission is completely free of vacuum hoses, fuel and coolant hoses, and electrical wiring.

1. Slowly raise the engine about 150 mm (6 in.). Check once again that all hoses and electrical wiring are disconnected from the engine/transmission.

1. Raise the engine all the way, and remove it from the vehicle.