1. Check for continuity between fuel pump 5P connector terminal No. 5 and body ground.

Is there continuity?

YES | - | Replace PGM-FI main relay 2 (FUEL PUMP). Also replace the No. 19 FUEL PUMP (15 A) fuse.■
NO | - | Check the fuel pump, and replace it if necessary. Also replace the No. 19 FUEL PUMP (15 A) fuse.■

1. Jump the SCS line with the HDS.

1. Disconnect ECM/PCM connector E (31P).

1. Turn the ignition switch ON (II).