1. Tighten the nuts (A) by the hand with a new high pressure pipe.

1. Tighten the fuel pump.

1. Tighten the nut of fuel pump side (B).

1. Tighten the nut of fuel rail side (C).

1. Install the parts in the reverse order of removal with a new injector fuel return hose assembly, and bleed the fuel system.
   NOTE:
   - If the high pressure pipe clamp and rubber (C) are is not installed, fuel may leak from fuel pipe.
   - If the O-ring is damage, replace the injector return hose assembly.