1. Check for continuity between the No. 2 terminal of the A/C compressor clutch relay 4P socket and the No. 1 terminal of the A/C compressor clutch 1P connector.

Is there continuity?

YES | - | Check the A/C compressor clutch clearance, and the A/C compressor clutch field coil. Repair as needed.■
NO | - | Repair open in the wire between the A/C compressor clutch relay and the A/C compressor clutch.■