Design Specifications

Item | Measurement | Qualification | Specification
--- | --- | --- | ---
DIMENSIONS | Overall length |  | 4,665 mm (183.7 in.)
Overall width |  | 1,760 mm (69.3 in.)
Overall height |  | 1,445 mm (56.9 in.)
Wheel base |  | 2,680 mm (105.5 in.)
Track | Front | 1,515 mm (59.6 in.)
Rear | 1,525 mm (60.0 in.)
Seating capacity |  | Five (5)
WEIGHT | Curb weight |  | 1,463−1,533 kg (3,225−3,380 lbs)
Max. permissible weight |  | 1,970 kg (4,343 lbs)
ENGINE | Type |  | Water-cooled, 4-stroke DOHC intercooler turbo diesel engine
Cylinder arrangement |  | Inline 4-cylinder, transverse
Bore and stroke |  | 85.0 x 97.1 mm (3.35 x 3.82 in.)
Displacement |  | 2,204 cm 3 (134.5 cu in.)
Compression ratio |  | 16.7
Valve train |  | Chain driven, DOHC 4 valves per cylinder
Lubrication system |  | Forced, wet sump, with trochoid pump
Oil pump displacement | At 4,000 rpm (min −1 ) | 52.2 L (55.2 US qt, 45.9 Imp qt)/minute
Water pump displacement | At 6,000 rpm (min −1 ) | 215 L (227 US qt, 189 Imp qt)/minute
Fuel required |  | EC REF. Fuel
STARTER | Type |  | Gear reduction
Normal output |  | 2.0 kW
Nominal voltage |  | 12 V
Hour rating |  | 30 seconds
Rotation direction |  | Clockwise as viewed from gear end
CLUTCH | Clutch type |  | Single plate dry, diaphragm spring
Clutch friction material surface area |  | 203 cm 2 (31.5 sq in.)
MANUAL TRANSMISSION | Type | AWD6 | Synchronized, 5-speed forward, 1 reverse
Primary reduction |  | Direct 1:1
Gear ratio | 1st | 3.933
2nd | 2.037
3rd | 1.250
4th | 0.883
5th | 0.687
Reverse | 4.008
Final reduction | Type | Single helical gear
Gear ratio | 3.285

(cont'd)

Item | Measurement | Qualification | Specification
--- | --- | --- | ---
STEERING | Type |  | Power-assisted rack and pinion
Overall ratio |  | 14.57
Turns, lock-to-lock |  | 2.85
Steering wheel diameter |  | 380 mm (15.0 in.)
SUSPENSION | Type | Front | Independent double wishbone with stabilizer, coil sprig
Rear | Independent double wishbone with stabilizer, coil sprig
Shock absorber | Front | Telescopic, hydraulic, nitrogen gas-filled
Rear | Telescopic, hydraulic, nitrogen gas-filled
BRAKES | Type of service brake | Front | Power-assisted self-adjusting ventilated disc
Rear | Power-assisted self-adjusting solid disc
Type of parking brake |  | Mechanical actuating, rear wheels
Pad friction surface area | Front | 48.8 cm 2 x 2 (7.56 sq in. x 2)
Rear | 24.3 cm 2 x 2 (3.77 sq in. x 2)
TYRES | Size |  | See tyre information label.
AIR CONDITIONING | Compressor | Type | Swash plate
Capacity | 188 mL (11.47 cu in.)/rev.
Maximum speed | 8,400 rpm (min −1 )
Lubricant capacity | 160 mL (5 1/3 fl oz)
Lubricant type | DENSO ND-OIL 8
Condenser | Type | Corrugated fin
Evaporator | Type | Corrugated fin
Blower | Type | Radial
Motor type | 210 W/12 V
Speed control | Infinite variable
Maximum capacity | 485 m 3 /h (17,100 cu ft/h)
Temperature control |  | Air-mix type
Compressor clutch | Type | Dry, signal plate, poly V-belt drive
Electrical power consumption at 20 °C (68 °F) | 48 W maximum at 12 V
Refrigerant | Type | HFC-134a (R-134a)
Capacity | 450−500 g (15.9−17.6 oz)
ELECTRICAL RATINGS | Battery |  | 12 V−59 AH/5 hours
Starter |  | 12 V−2.0 kW
Alternator |  | 12 V−105 A
Fuses | Under-hood fuse/relay box | 100 A, 70 A, 50 A, 40 A, 30 A, 20 A, 15 A, 10 A, 7.5 A
Under-dash fuse/relay box | 30 A, 20 A, 15 A, 10 A, 7.5 A
Multi-fuel relay box | 30 A, 7.5 A
Light bulbs | Headlight high beam | 12 V−60 W (HB3)
Headlight low beam | 12 V−55 W (HB4)
12 V−35 W (HID)
Front fog lights | 12 V−55 W
Front turn signal lights | 12 V−21 W
Front parking lights | 12 V−5 W
Side turn signal lights | LED
Rear turn signal lights | 12 V−21 W
Stop/taillights | 12 V−21/5 W
Taillights | 12 V−5 W
High-mount brake light | 12 V−21 W
Back-up lights | 12 V−21 W
License plate light | 12 V−5 W
Rear fog lights | 12 V−21 W
Ceiling light | 12 V−8 W
Spotlights | 12 V−8 W
Trunk light | 12 V−5 W
Door courtesy lights | 12 V−3.8 W
Glove box light | 12 V−3.4 W
Vanity mirror lights | 12 V−2 W
Gauge lights | LED
Indicator lights | LED