1. Carefully pull the adhesive backing away, and push the molding (A) against the rear pillar to stick the adhesive tape (B).

1. Spray water over the quarter glass and check for leaks. Mark the leaking areas and let the quarter glass dry, then seal with sealant. Let the vehicle stand for at least 4 hours after quarter glass installation. If the vehicle has to be used within the first 4 hours, it must be driven slowly.

1. Reinstall all remaining removed parts.
   NOTE: Advise the customer not to do the following things for 2 to 3 days:
   - Slam the doors with all the windows rolled up.
   - Twist the body excessively (such as when going in and out of driveways at an angle or driving over rough, uneven roads).