1. Disconnect the A/T clutch pressure control solenoid valves B and C connectors.

1. Measure A/T clutch pressure control solenoid valve B resistance between the solenoid valve B terminals No. 1 and No. 2, and measure A/T clutch pressure control solenoid valve C resistance between the solenoid valve C terminals No. 1 and No. 2.

   Standard: | 3−10 Ω

1. If the resistance of either A/T clutch pressure control solenoid valve is out of standard, replace the A/T clutch pressure control solenoid valves B and C.

1. Connect the battery positive terminal to the No. 1 terminal of the A/T clutch pressure control solenoid valves B and C connectors, and connect the battery negative terminal to the No. 2 terminal. A clicking sound should be heard.

1. If no sound is heard, remove the A/T clutch pressure control solenoid valves B and C.

1. Check the fluid passage of the A/T clutch pressure control solenoid valve for dust or dirt.