NOTE:

- Take care not to tear the seams or damage the seat covers.
- Put on gloves to protect your hands.

1. Tilt the seat-back half-way forward, and tip the seat cushion up.

1. Remove these items:
   - Headrest and center headrest
   - Cargo net (for some models)
   - Seat-back top cover
   - Armrest (right seat-back)

1. Release the clips fastening the seat-back cover as needed, and unzip the cover.

1. Right seat-back: Remove the center headrest guides from the seat-back.

1. Recline the seat-back fully, and secure it. Pull out the seat belt (A) and center seat belt (B) (right seat-back) as needed, then pull out the seat-back cover/pad (C) from the frame (D).