1. Install the seat belt in the reverse order of removal, and note these items:
   - Apply liquid thread lock to the upper anchor bolt before reinstallation.
   - Check that the retractor locking mechanism functions.
   - Assemble the washers, collars, and bushings on the upper and lower anchor bolts as shown.
   - Before installing the anchor bolts, make sure there are no twists or kinks in the front seat belt.
   - Make sure the seat belt tensioner connector is plugged in properly.
   - Reconnect the negative cable to the battery.
   - Reset the clock.
   - Perform the power window control unit reset procedure.

Upper anchor bolt construction
Lower anchor bolt construction