1. Remove the shift solenoid harness connector.

1. Measure ATF temperature sensor resistance between shift solenoid harness connector terminals No. 6 and No. 7.

   Standard: | 50 Ω−25 kΩ

1. If the resistance is out of standard, replace the ATF temperature sensor and solenoid harness; go to Step 17 . The ATF temperature sensor is not available separately from the solenoid harness.
   If the measurement is within the standard, install the removed parts; go to Step 20 .

1. Disconnect the connectors from the shift solenoid valves.