1. Check cable free play at the throttle linkage. Cable free pley (A) should be 15−18 mm (9/16−11/16 in.).

1. If the free play is not within spec 15−18 mm (9/16−11/16 in.), loosen the locknut (B), turn the adjusting nut (C) until the deflection is as specified, then retighten the locknut.

1. With the cable properly adjusted, check the throttle link to be sure it opens fully when you push the accelerator pedal to the floor. Also check the throttle link to be sure it returns whenever you release the accelerator pedal.