Rear Suspension Stabilizer Bar Replacement

1. Raise the rear of the vehicle, and support it with safety stands in the proper locations.

1. Remove the rear wheels.

1. Disconnect the stabilizer links from the stabilizer bar (A) on the right and left sides.

1. Remove the flange bolts and bushing holders (B), then remove the bushing (C) and the stabilizer bar.

1. Install the stabilizer bar in the reverse order of removal, and note these items:
   - Note the right and left direction of the stabilizer bar.
   - Align the ends of the paint marks (A) on the stabilizer bar with the bushing (B).
   - Refer to Stabilizer Link Replacement to connect the stabilizer to the links.