1. Place the several shop towel under the line connections, and cover the gearbox mounting part to protect it from the power steering fluid. Loosen the flare nut (A), and disconnect the feed line (B).

1. Loosen the flare nut (C), and disconnect the return line (D).

1. After disconnecting the lines, plug or seal them with a piece of tape or equivalent to prevent foreign materials from entering.
   NOTE: Do not loosen the cylinder line A and B between the valve body unit and cylinder.