1. Loosely install the flange bolt (A) on the bottom of the damper. Connect the stabilizer link (B) on the bracket (C), and loosely install the flange nut (D).

1. Raise the rear suspension with a floor jack to load the vehicle weight, and tighten the flange bolt to the specified torque.

1. Tighten the flange nut while holding the joint pin (E) with a hex wrench (F).

1. Tighten the two flange nuts on top of the damper to the specified torque.

1. Install the rear piller trim without side curtain airbag models, with side curtain airbag models.

1. Install the seat side bolster.

1. Clean the mating surface of the brake disc and the inside of the wheel, then install the rear wheel.

1. Check the wheel alignment, and adjust it if necessary.