1. Remove the upper balancer shaft holder and bearings again, then measure the widest part of the plastigage. If the balancer shaft No. 2 journal oil clearance is out-of-tolerance, install new bearings, and recheck. If it is still out-of-tolerance; replace the balancer shafts.

   No. 2 Journal Oil Clearance
   Standard (New): | 0.060−0.120 mm (0.0024−0.0047 in.)
   Service Limit: | 0.15 mm (0.006 in.)