ABS indicator does not go off, and no DTCs are stored

1. Disconnect the ABS control unit 25P connector.

1. Turn the ignition switch ON (II).

1. Measure the voltage between the ABS control unit 25P connector terminal No. 16 and body ground.

Is there battery voltage?

YES | - | Go to Step 4 .
NO | - | Repair open in the wire between the No. 18 (15 A) fuse and the ABS modulator-control unit.■

1. Turn the ignition switch OFF.