Audio Unit Connector Replacement - Without Premium Audio

When replacing an audio unit connector, match the wires to the cavities listed in the following table.

Cavity | Wire | Connect to | Cavity | Wire | Connect to
--- | --- | --- | --- | --- | ---
A1 | YEL/GRN | Radio switch (AMP.) | A11 | BRN | Radio remote switch ground
A2 | RED | ACC (main stereo power supply) | A12 | ——— | Not used
A3 | PUR[GRN/RED] | Radio remote switch | A13 | ——— | Not used
A4 | RED[RED/BLU] | (Security input) | A14 | ——— | Not used
A5 | PNK | Right rear speaker (+) | A15 | BLU/YEL | Right rear speaker (−)
A6 | BLU/WHT | Left rear speaker (+) | A16 | BLU/BLK | Left rear speaker (−)
A7 | GRN/YEL | Front passenger's door speaker (+), Right tweeter (+) | A17 | GRY | Front passenger's door speaker (−), Right tweeter (−)
A8 | GRN/BLK | Driver's door speaker (+), Left tweeter (+) | A18 | LT GRN | Driver's door speaker (−), Left tweeter (−)
A9 | RED/BLK | Lights-on signal | A19 | RED | Dash lights brightness controller
A10 | WHT | Constant power | A20 | BLK | Ground (G504)

[ ]: | RHD type

Without Navigation, Premium Audio