1. Connect the HDS to the DLC (A).

1. Choose Clutch Pressure Control (Linear) Solenoid A in Miscellaneous Test Menu on the HDS.

1. Test the A/T clutch pressure control solenoid valve A with the HDS.

1. Follow instructions indicated on the HDS by the test result. If the HDS has not determined the cause of the failure, remove A/T clutch pressure control solenoid valve A and test.

1. Remove the intake air duct.