NOTE: Keep the cam chain away from magnetic fields.

1. Remove the cylinder head cover.

1. Set up the No. 1 piston at top dead center (TDC). The ‘‘UP'' mark (A) on the cam chain sprocket should be at the top. Align the TDC marks (B) on the intake camshaft gear and the exhaust camshaft gear.

1. Remove the right front tyre/wheel.

1. Remove the splash shield.

1. Remove the drive belt.

1. Remove the crankshaft pulley.

1. Support the engine with a jack and wood block under the oil pan.