1. Remove the upper balancer shaft holder and bearings again, and measure the widest part of the plastigage.
   If the balancer shaft No. 3 journal oil clearance is out-of-tolerance, install new bearings, and recheck. If it still out-of-tolerance; replace the balancer shafts.

   No. 3 Journal Oil Clearance
   Standard (New): | 0.060−0.120 mm
   (0.0024−0.0047 in.)
   Service Limit: | 0.15 mm (0.006 in.)