NOTE: After this inspection, you must select engine control module (ECM)/powertrain control module (PCM) reset, using the Honda Diagnostic System (HDS), otherwise ECM/PCM continues to stop the fuel injectors.

1. Warm up the engine to normal operating temperature (cooling fan comes on).

1. Turn the ignition switch OFF.

1. Connect the HDS to the data link connector (DLC).

1. Select PGM-FI, INSPECTION, and then ALL INJECTORS OFF on the HDS.

1. Remove the four ignition coils.

1. Remove the four spark plugs.

1. Attach the compression gauge to the spark plug hole.

1. Open the throttle fully, then crank the engine with the starter motor and measure the compression.

   Compression Pressure:
   Above 930 kPa (9.5 kgf/cm 2 , 135 psi)

1. Measure the compression on the remaining cylinders.

   Maximum Variation:
   Within 200 kPa (2.0 kgf/cm 2 , 28 psi)

1. If the compression is not within specifications, check the following items, then remeasure the compression.
   - Damaged or worn valves and seats
   - Damaged cylinder head gasket
   - Damaged or worn piston rings
   - Damaged or worn piston and cylinder bore

1. Select ECM/PCM reset to cancel the ALL INJECTORS OFF function on the HDS.