Engine idle

Item | Measurement | Qualification | Standard or New
--- | --- | --- | ---
Engine idle | Idle speed with no load | K20A6 (M/T) M/T in neutral | 650±50 rpm (min −1 )
K20A6 (A/T) A/T in N or P position | 650±50 rpm (min −1 )
K24A3 (M/T) M/T in neutral | 600±50 rpm (min −1 )
K24A3 (A/T) A/T in N or P position | 650±50 rpm (min −1 )
Idle speed with high electric load (A/C switch ON, temperature set to Max Cool, blower fan on High, rear window defogger ON, and headlights on high beam) | K20A6 (M/T) M/T in neutral | 720±50 rpm (min −1 )
K20A6 (A/T) A/T in N or P position | 800±50 rpm (min −1 )
K24A3 (M/T) M/T in neutral | 720±50 rpm (min −1 )
K24A3 (A/T) A/T in N or P position | 800±50 rpm (min −1 )
Idle CO |  | 0.1 % max.