Special Tools Required Handle driver 07749-0010000 Driver attachment, 78 x 90 mm 07GAD-SD40101
Driver attachment, 72 x 75 mm
07746-0010600
NOTE:

- The bearing and bearing outer race should be replaced as a set.
- Replace the bearing with a new one whenever the outer race is replaced.
- Do not use the thrust shim on the torque converter housing.
- Adjust bearing preload after replacing the bearing and outer race.
- Coat all parts with ATF during installation.

1. Remove the bearing outer race (A), 76.2 mm thrust washer (B), and 76 mm thrust shim (C) from the transmission housing (D) by heating the housing to about 100 °C (212 °F) with a heat gun (E). Do not heat the housing more than 100 °C (212 °F).
   NOTE: Let the transmission housing cool to room temperature before installing the bearing outer race.