1. Bleed the clutch hydraulic system.
   - Attach a hose to the bleeder screw (A), and suspend the hose in a container of brake fluid.
   - Make sure there is an adequate supply of fluid in the clutch master cylinder, then slowly pump the clutch pedal until no more bubbles appear at the bleeder hose.
   - It may be necessary to limit the movement of the release fork (B) with a block of wood to remove all the air from the system.
   - Tighten the bleeder screw to 8 N·m (0.8 kgf·m, 5.8 lbf·ft); do not overtighten it.
   - Refill the clutch master cylinder with fluid when done.
   - Always use only Honda DOT 3 or 4 brake fluid.

1. Install the air cleaner housing.

1. Reconnect the battery cables; positive (+) cable first, then the negative (−) cable.

1. Enter the anti-theft code for the radio and navigation system, then enter the customer's radio station presets.

1. Perform the power window control unit reset procedure.