1. Apply a light coat of primer, then apply a double-sided adhesive tape (A) to the molding (B) as shown. Attach the fastener (C) with adhesive tape to the inside face of the quarter glass (D):
   - Be sure the fastener lines up with the alignment marks (E).
   - Be careful not to touch the quarter glass where adhesive will be applied.
   - Do not peel the separators off the double-sided adhesive tape.

   Double-sided adhesive tape:
   | Thickness 0.6 mm (0.02 in.)
   | Width 4 mm (0.16 in.)
   Fastener adhesive tape:
   | Thickness 0.6 mm (0.02 in.)
   | Width 7.5 mm (0.3 in.)