Alternator Replacement

1. Make sure you have the anti-theft codes for the radio and navigation system, then write down the customer's radio station presets.

1. Disconnect the negative cable from the battery first, then disconnect the positive cable.

1. Remove the drive belt.

1. Remove the two bolts securing the expansion tank (A), then move the expansion tank.

1. Disconnect the A/C condenser fan motor connector (A).

1. Remove the two bolts (B), and loosen the two bolts (C) securing the A/C condenser fan shroud, then remove the A/C condenser fan shroud assembly (D).

1. Disconnect the alternator connector (A) and BLK wire (B), and remove the harness clamp (C) from the alternator.

1. Remove the four bolts, then remove the alternator oil shield (A) and alternator (B).

1. Install the alternator in the reverse order of removal.

1. Connect the positive cable to the battery first, then connect the negative cable.

1. Enter the anti-theft code for the radio and navigation system, then enter the customer's radio station presets.

1. Set the clock.

1. Do the power window control unit reset procedure.