1. Install the damper forks (A) with damper pinch bolts (B) and new self-locking nuts (C), then install the ball joints on the lower arms (D) with the castle nuts (E) and new cotter pins (F).
   NOTE: Be careful not to damage the headlight adjuster leveling sensor arm.

1. Install the stabilizer links (G) to the lower arms, and install the nuts (H). Insert a 6 mm Allen wrench (I) in the ball joint pin (J), and tighten the nuts.