1. Install the headliner in the reverse order of removal, and note these items:
   - If the side curtain airbag has been deployed, replace the headliner and grab handle on deployed side with new ones.
   - To prevent the side curtain airbags from deploying improperly and possibly causing injury, inspect removed pieces and replace them if they have any of these types of damage:

   - | Any creases or tears in the headliner (A)
   - | Any fasteners (B) which have come off the headliner
   - | Any damage around the grab handle holes (C) or sunvisor holes (D) in the headliner
   - | Any deformations in the grab handle (E)
   - | Any cracks in the sunvisor stay base (F)
   - | Any bends or cracks in the sunvisor stay shaft (G)
   - | Any cracks in the sunvisor base (H)
   - | Any cracks in the vanity mirror base (I)
   - | Any deformations in the grab handle bracket

   - Replace any damaged parts with new ones.
   - Make sure the top of the headliner overlaps with the trim pieces correctly.
   - When passing the headliner through the door opening, be careful not to fold or bend it. Also, be careful not to scratch the body.
   - If the threads on a visor or grab handle screw is worn out, use an oversized self-tapping ET screw made specifically for this application:
     Visor: P/N 90137-S30-003
     Grab handle: P/N 90137-S0A-003
   - Check that both sides of the headliner are securely attached to the trim.

Headliner
Grab handle
Sunvisor