DTC P0335: CKP Sensor No Signal

1. Turn the ignition switch ON (II).

1. Clear the DTC with the HDS.

1. Start the engine. If engine does not start, keep cranking for 10 seconds.

1. Check for Temporary DTCs or DTCs with the HDS.

Is DTC P0335 indicated?

YES | - | Go to Step 5 .
NO | - | Intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the CKP sensor and the ECM.■

1. Turn the ignition switch OFF, and wait 30 seconds.

1. Disconnect the CKP sensor 3P connector.

1. At sensor side, measure resistance between CKP sensor 3P connector terminals No. 2 and No. 3.

Is there about 15.6 kΩ at room temperature?

YES | - | Go to Step 8 .
NO | - | Go to Step 15 .

1. Disconnect ECM connector No. 1 (96P).