1. Lift up the front seat, then detach the harness clip (A), and disconnect the seat belt switch connector (B) on the manual height adjustable seat, the power seat harness connector (C) on the driver's and passenger's power seats, if equipped, the seat heater connector (D) except on the power seat, the side airbag connector (E) on the driver's and passenger's seat, and the OPDS unit connector (F) on the passenger's seat.
   NOTE:
   - LHD is shown; RHD is symmetrical.
   - 4-way power seat on LHD model is symmetrical to RHD model, but it has no OPDS unit.

1. With the help of an assistant, carefully remove the front seat through the front door opening.

Manual seat without OPDS unit
Manual seat with OPDS unit (RHD)
Manual height adjustable seat
4-way power seat with OPDS unit (RHD)
8-way power seat