How to Remove the ECM for Testing If DTC troubleshooting requires voltage or resistance checks at the ECM connectors, remove the ECM and test it:

1. Turn the ignition switch OFF, and wait 30 seconds.

1. Remove the passenger's kick panel.

1. Disconnect the ECM connectors (A).

1. Loosen the bolts (B).

1. Remove the bolts (C), then remove the ECM (D).

1. Install the ECM in the reverse order of removal.