Special Toolds Required Keyless Entry Checker 07MAJ-SP00400 NOTE:

- If the doors unlock or lock with the transmitter, but the LED on the trnsmitter dose not come on, the LED is faulty; replace the transmitter.
- If any door is open, you cannot lock the doors with the transmitter.
- If you unlock the doors with the transmitter, but do not open any of the doors within 30 seconds, the doors relock automatically.
- The doors do not lock or unlock with the transmitter if the ignition key inserted in the ignition switch.

1. Put on transmitter (A) behind the keyless entry checker (B).

1. Press the door lock button.
   - If the indicator light comes on, the transmitter is OK.
   - If the indicator light dose not come on, check for:

   - | a dead or low battery.
   - | faulty transmitter.