1. Push in the piston (A) so that the caliper will fit over the pads. Make sure the pin boot is in position to prevent damaging it when pivoting the caliper down.

1. Pivot the caliper (B) down into position. Install the flange bolt (C), and tighten it to the specified torque while holding the pin (D) with a wrench being careful not to damage the pin boot.

1. Press the brake pedal several times to make sure the brakes work, then test-drive the vehicle.
   NOTE: Engagement of the brake may require a greater pedal stroke immediately after the brake pads have been replaced as a set. Several applications of the brake pedal will restore the normal pedal stroke.

1. After installation, check for leaks at hose and line joints or connections, and retighten if necessary.

1. Install the rear wheels.