1. Install the ground cable (A), then install the battery base (B).

1. Install the air cleaner housing.

1. Install the battery. Connect the positive (+) cable first, then the negative (−) cable to the battery.

1. Refill the transmission fluid.

1. Test-drive the vehicle.

1. Check the clutch operation.

1. Shift into the 5th gear. Make sure the transmission does not shift direct into the reverse gear (Then return to Neutral position, and enable to shift into reverse gear).

1. Check the front wheel alignment.

1. Enter the anti-theft code for the audio and navigation system, then enter the customer's audio presets.

1. Do the power window control unit reset procedure.