NOTE:

- Take care not to scratch the dashboard and related parts.
- When prying components, use the handy remover set or equivalent.
- LHD is shown; RHD is symmetrical.

1. Adjust the steering column upward.

1. Remove the screw (A) securing the dashboard lower cover (B). Starting at the left lower corner working toward the right, gently pull out the bottom to detach four clips (C) and a hook (D). Disconnect the VSA switch connector (E), and if equipped, headlight adjuster switch connector (F).