DTC P0341: CMP Sensor and CKP Sensor Incorrect Phase Detected

1. Turn the ignition switch ON (II).

1. Clear the DTC with the HDS.

1. Test-drive at a steady speed between 30−60 km/h (19−38 mph) for 10 minutes.

1. Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS.

Is DTC P0341 indicated?

YES | - | Go to Step 9 .
NO | - | Go to Step 5 .

1. Do the VTC TEST in the INSPECTION MENU with the HDS.

Is the result OK?

YES | - | Go to Step 6 .
NO | - | Go to Step 9 .

1. Test-drive at a steady speed between 30−60 km/h (19−38 mph) for 10 minutes.

1. Check the VTC STATUS in the DATA LIST with the HDS.

Does it indicate ON?

YES | - | Go to Step 8 .
NO | - | Go to Step 6 and recheck.

1. Monitor the OBD STATUS for DTC P0341 in the DTCs MENU with the HDS.

Does the screen indicate FAILED?

YES | - | Go to Step 9 .
NO | - | If the screen indicates PASSED, intermittent failure, system is OK at this time. Check for poor connections or loose terminals at the VTC oil control solenoid valve and the ECM/PCM. If the screen indicates NOT COMPLETED, go to Step 6 and recheck.

1. Turn the ignition switch OFF.

1. Test the VTC oil control solenoid valve.

Is the VTC oil control solenoid valve OK?

YES | - | Go to Step 11 .
NO | - | Replace the VTC oil control solenoid valve, then go to Step 14 .

1. Check the camshaft timing.

Is the camshaft timing OK?

YES | - | Go to Step 12 .
NO | - | Time the camshaft, then go to Step 14 .

1. Check for damage to the cam chain.

Is the cam chain damaged?

YES | - | Replace the cam chain, then go to Step 14 .
NO | - | Go to Step 13 .

1. Inspect the VTC actuator.

Is the result OK?

YES | - | Go to Step 14 .
NO | - | Replace the VTC actuator, then go to Step 14 .

1. Turn the ignition switch ON (II).

1. Reset the ECM/PCM with the HDS.

1. Clear the CKP pattern with the HDS.

1. Do the ECM/PCM idle learn procedure.

1. Do the CKP pattern learn procedure.

1. Test-drive at a steady speed between 30−60 km/h (19−38 mph) for 10 minutes.

1. Check for Temporary DTCs or DTCs in the DTCs MENU with the HDS.

Are any Temporary DTCs or DTCs indicated?

YES | - | If DTC P0341 is indicated, check for poor connections or loose terminals at the VTC oil control solenoid valve and the ECM/PCM, then go to Step 1 . If any other Temporary DTCs or DTCs are indicated, go to the indicated DTC's troubleshooting.
NO | - | Go to Step 21 .

1. Monitor the OBD STATUS for DTC P0341 in the DTCs MENU with the HDS.

Does the screen indicate PASSED?

YES | - | Troubleshooting is complete.■
NO | - | If the screen indicates FAILED, check for poor connections or loose terminals at the VTC oil control solenoid valve and the ECM/PCM, then go to Step 1 . If the screen indicates NOT COMPLETED, go to Step 19 and recheck.