NOTE:

- Put on gloves to protect your hands.
- Wear eye protection while cutting the glass adhesive with piano wire.
- Use seat covers to avoid damaging any surfaces.
- Do not damage the rear window defogger grid lines, window antenna grid lines, and terminals.
- Use glass adhesive set P/N 08C73-X0230N.

1. Remove these items:
   - Trunk lid
   - Rear shelf

1. Disconnect the window antenna connectors (A) and rear window defogger connectors (B).

1. If the old rear window is to be reinstalled, make alignment marks across the glass and body with a grease pencil.