EPS Control Unit Inputs and Outputs for Connector B (2P)

Terminal number | Wire color | Terminal sign (Terminal name) | Description | Measurement
--- | --- | --- | --- | ---
Terminals | Conditions (Ignition Switch ON (II)) | Voltage
1 | WHT | +B (Plus battery) | Power source for the actuator motor | 1−GND | At all times | Battery voltage
2 | BLK | PG (Power ground) | Ground for the actuator motor | 2−GND | ——— | ———