NOTE:

- Use fender covers to avoid damaging painted surfaces.
- To avoid damaging the wire and terminals, unplug the wiring connectors carefully while holding the connector portion.
- To avoid damaging the cylinder head, wait until the engine coolant temperature drops below 38 °C (100 °F) before loosening the cylinder head bolts.
- Mark all wiring and hoses to avoid misconnection. Also, be sure that they do not contact other wiring or hoses, or interfere with other parts.

1. Relieve fuel pressure.

1. Drain the engine coolant.

1. Remove the fuel feed hose.

1. Remove the drive belt.

1. Disconnect the intake air temperature (IAT) sensor connector (A).

1. Remove the vacuum hose (B) and breather pipe (C), then remove the intake air duct (D).