1. Install the baffle plates.

1. Install the oil pump.

1. Install the oil pan.

1. Install the cylinder head.

1. M/T model: Install the flywheel, clutch disc, and pressure plate.

1. A/T model: Install the drive plate.

1. Install the transmission:
   - Manual transmission
   - Automatic transmission

1. Install the engine assembly.
   NOTE: Whenever any crankshaft or connecting rod bearing is replaced, it is necessary after reassembly to run the engine at idling speed until it reaches normal operating temperature, then continue to run it for about 15 minutes.