1. Disconnect the dashboard wire harness 4P connector (A) from the cable reel.

1. Connect the SRS inflator simulator (2 Ω connectors) and simulator lead F to the dashboard wire harness.

1. Reconnect the battery negative cable.

1. Erase the DTC memory.

1. Read the DTC.

Is DTC 11-3x indicated?

YES | - | Go to Step 15 .
NO | - | Short in the cable reel; replace the cable reel. ■

1. Turn the ignition switch OFF. Disconnect the battery negative cable, and wait for 3 minutes.