1. Connect the No. 1 terminal of the A/C condenser fan 2P connector to body ground with jumper wire.

1. Turn the ignition switch ON (II), then turn the A/C and fan switches ON.

Does the A/C condenser fan run?

YES | - | Go to Step 29 .
NO | - | Replace the A/C condenser fan motor.■

1. Turn the A/C and fan switches OFF, then turn the ignition switch OFF.

1. Disconnect the jumper wire.

1. Remove the fan control relay from the multi-relay box, and test it.

Is the relay OK?

YES | - | Go to Step 32 .
NO | - | Replace the fan control relay.■

1. Turn the ignition switch ON (II), then turn the A/C and fan switches ON.