1. Check for continuity between A/T clutch pressure control solenoid valve C connector terminal No. 2 and body ground.

Is there continuity?

YES | - | Update the PCM if it does not have the latest software, or substitute a known-good PCM, then recheck. If the symptom/indication goes away with a known-good PCM, replace the original PCM .■
NO | - | Repair open in the wire between the A/T clutch pressure control solenoid valve C and ground (G101), or repair poor ground (G101), then go to Step 10 .

1. Clear the DTC with the HDS.

1. Test-drive the vehicle for several minutes in the D position in all five gears.

1. Monitor the OBD status for P0971 in the DTCs/Freeze Data in A/T Mode Menu for a pass/fail.

Does the result indicate a pass?

YES | - | The problem has been corrected.■
NO | - | Return to Step 1 and recheck.■