NOTE:

- Once you remove the door outer molding, replace it with a new one because it will bend during removal.
- Put on gloves to protect your hands.
- Take care not to scratch the door.
- Use the handy remover set, or equivalent when prying components.

1. Pry the clip at each end with a handy remover.

1. While removing the upper edge of the door outer molding (A) from the edge of the sash, cut the double-sided adhesive tapes (B) with a utility knife, then remove the molding.

1. Scrape off the remaining double-sided adhesive tape from the sash, then clean the sash surface with a sponge dampened in alcohol.

1. Install a new door outer molding in the reverse order of removal, and note these items.
   - Push the clip and the adhesive portions into place securely.
   - Make sure the upper and lower sides of the molding are catching the edges of the sash properly.