1. Install the drive belt (A).
   Note these item during belt installation:
   - Make sure that the belt is properly positioned on the pulleys (B).
   - Do not get power steering fluid or grease on the auto-tensioner, alternator, A/C compressor, and drive belt or pulley faces. Clean off any fluid or grease before installation.

1. Tighten the pump mounting bolts to the specified torque.

1. Fill the reservoir to the upper level line.